    PAD Specification File
    ***************************

    PART TYPE:        LFCPNX-100
    Performance Grade:      9_High-Performance_1.0V
    PACKAGE:          BBG484
    Package Status:                     Final          Version 16

    Mon Mar 18 12:42:55 2024

    Pinout by Port Name:
    +---------------+----------+---------------+--------+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | Port Name     | Pin/Bank | Buffer Type   | Site   | Properties                                                                                                                                                               |
    +---------------+----------+---------------+--------+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | LED[0]        | L10/7    | LVCMOS33_BIDI | PL24B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[10]       | R1/6     | LVCMOS33_BIDI | PL60A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[11]       | R7/6     | LVCMOS33_BIDI | PL65A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[1]        | L13/2    | LVCMOS33_BIDI | PR40B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[2]        | L9/7     | LVCMOS33_BIDI | PL26A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[3]        | L14/2    | LVCMOS33_BIDI | PR40A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[4]        | J7/7     | LVCMOS33_BIDI | PL13A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[5]        | L12/2    | LVCMOS33_BIDI | PR42A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[6]        | J6/7     | LVCMOS33_BIDI | PL13B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[7]        | L11/7    | LVCMOS33_BIDI | PL24A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[8]        | M5/7     | LVCMOS33_BIDI | PL38B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | LED[9]        | M6/6     | LVCMOS33_BIDI | PL40A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF        |
    | clk_ext       | J14/1    | LVCMOS33_IN   | PR10A  | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF          |
    | cmos_xclr     | M17/2    | LVCMOS33_OUT  | PR47A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | ddr_ca_o[0]   | Y7/4     | LVSTL_I_OUT   | PB50B  | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | ddr_ca_o[1]   | W7/4     | LVSTL_I_OUT   | PB50A  | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | ddr_ca_o[2]   | AA21/3   | LVSTL_I_OUT   | PB154B | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | ddr_ca_o[3]   | AB19/3   | LVSTL_I_OUT   | PB110B | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | ddr_ca_o[4]   | AB20/3   | LVSTL_I_OUT   | PB114B | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | ddr_ca_o[5]   | AB21/3   | LVSTL_I_OUT   | PB114A | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | ddr_ck_o[0]   | AA11/4   | LVSTLD_I_OUT  | PB92A  | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTLD_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF      |
    | ddr_cke_o[0]  | AB11/4   | LVSTL_I_OUT   | PB90A  | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | ddr_cs_o[0]   | AA13/4   | LVSTL_I_OUT   | PB94B  | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | ddr_dmi_io[0] | AA8/4    | LVSTL_I_BIDI  | PB62A  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dmi_io[1] | U15/3    | LVSTL_I_BIDI  | PB130A | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[0]  | T9/4     | LVSTL_I_BIDI  | PB64B  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[10] | V16/3    | LVSTL_I_BIDI  | PB132B | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[11] | W16/3    | LVSTL_I_BIDI  | PB132A | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[12] | AA15/3   | LVSTL_I_BIDI  | PB122A | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[13] | Y15/3    | LVSTL_I_BIDI  | PB124A | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[14] | AA16/3   | LVSTL_I_BIDI  | PB122B | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[15] | V15/3    | LVSTL_I_BIDI  | PB128A | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[1]  | T10/4    | LVSTL_I_BIDI  | PB80B  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[2]  | U10/4    | LVSTL_I_BIDI  | PB80A  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[3]  | AA9/4    | LVSTL_I_BIDI  | PB62B  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[4]  | AA10/4   | LVSTL_I_BIDI  | PB82A  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[5]  | W10/4    | LVSTL_I_BIDI  | PB84A  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[6]  | V10/4    | LVSTL_I_BIDI  | PB84B  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[7]  | Y10/4    | LVSTL_I_BIDI  | PB82B  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[8]  | Y16/3    | LVSTL_I_BIDI  | PB124B | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dq_io[9]  | W15/3    | LVSTL_I_BIDI  | PB128B | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:VREF_INT |
    | ddr_dqs_io[0] | AB9/4    | LVSTLD_I_BIDI | PB66A  | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTLD_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF     |
    | ddr_dqs_io[1] | AB16/3   | LVSTLD_I_BIDI | PB126A | DRIVE:10mA SLEWRATE:FAST GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTLD_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF     |
    | ddr_odt_ca_o  | M3/7     | LVCMOS33_OUT  | PL35B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | ddr_reset_n_o | Y21/3    | LVSTL_I_OUT   | PB154A | DRIVE:10mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTL_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF       |
    | fs[0]         | M4/7     | LVCMOS33_OUT  | PL38A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | fs[1]         | J1/7     | LVCMOS33_OUT  | PL10B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | fs[2]         | R9/6     | LVCMOS33_OUT  | PL67B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | gnd_clk       | M1/7     | LVCMOS33_OUT  | PL33B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | init_done_o   | L22/1    | LVCMOS33_OUT  | PR38B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | mipi_clk      | H14/1    | LVCMOS33_OUT  | PR8A   | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | out_clk0      | G5/7     | LVCMOS33_OUT  | PL6A   | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | out_clk1      | F19/0    | LVCMOS33_OUT  | PT148A | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | pll_refclk_i  | T2/5     | LVSTLD_I_IN   | PB2A   | DRIVE:NA SLEWRATE:NA GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVSTLD_I DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:ON VREF:OFF         |
    | rstn_i        | H22/1    | LVCMOS33_IN   | PR13B  | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF          |
    | sim_o         | R5/6     | LVCMOS33_OUT  | PL64A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    | uart_rxd_i    | F22/0    | LVCMOS33_IN   | PT156A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF          |
    | uart_txd_o    | F21/0    | LVCMOS33_OUT  | PT154B | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF      |
    +---------------+----------+---------------+--------+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 0    | 3.3V  |
    | 1    | 3.3V  |
    | 2    | 3.3V  |
    | 3    | 1.1V  |
    | 4    | 1.1V  |
    | 5    | 1.1V  |
    | 6    | 3.3V  |
    | 7    | 3.3V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +----------+-----------------------+------------+---------------+-----------------+----------------------------------------------------------+
    | Pin/Bank | Pin Info              | Preference | Buffer Type   | Site            | Dual Function                                            |
    +----------+-----------------------+------------+---------------+-----------------+----------------------------------------------------------+
    | A2/80    |                       |            |               | SD2_TXDP        |                                                          |
    | A3/80    |                       |            |               | SD2_TXDN        |                                                          |
    | A5/80    |                       |            |               | SD3_TXDP        |                                                          |
    | A6/80    |                       |            |               | SD3_TXDN        |                                                          |
    | A9/81    |                       |            |               | SD4_TXDP        |                                                          |
    | A10/81   |                       |            |               | SD4_TXDN        |                                                          |
    | A12/81   |                       |            |               | SD5_TXDP        |                                                          |
    | A13/81   |                       |            |               | SD5_TXDN        |                                                          |
    | A15/81   |                       |            |               | SD6_TXDP        |                                                          |
    | A16/81   |                       |            |               | SD6_TXDN        |                                                          |
    | A18/81   |                       |            |               | SD7_TXDP        |                                                          |
    | A19/81   |                       |            |               | SD7_TXDN        |                                                          |
    | A21/83   |                       |            |               | SD_EXT1_REFCLKP |                                                          |
    | AA1/5    |     unused, PULL:DOWN |            |               | PB42B           | BDQSN42                                                  |
    | AA2/5    |     unused, PULL:DOWN |            |               | PB38A           | BDQ42                                                    |
    | AA3/5    |     unused, PULL:DOWN |            |               | PB38B           | BDQ42                                                    |
    | AA4/5    |     unused, PULL:DOWN |            |               | PB44A           | BDQ42                                                    |
    | AA5/5    |     unused, PULL:DOWN |            |               | PB46A           | PCLKT5_3/BDQ42                                           |
    | AA6/5    |     unused, PULL:DOWN |            |               | PB48B           | VREF5_2/BDQ42                                            |
    | AA7/4    |     unused, PULL:DOWN |            |               | PB58A           | PCLKT4_1/BDQ54                                           |
    | AA8/4    | ddr_dmi_io[0]         | LOCATED    | LVSTL_I_BIDI  | PB62A           | BDQ66                                                    |
    | AA9/4    | ddr_dq_io[3]          | LOCATED    | LVSTL_I_BIDI  | PB62B           | BDQ66                                                    |
    | AA10/4   | ddr_dq_io[4]          | LOCATED    | LVSTL_I_BIDI  | PB82A           | BDQ66                                                    |
    | AA11/4   | ddr_ck_o[0]+          | LOCATED    | LVSTLD_I_OUT  | PB92A           | BDQ90                                                    |
    | AA12/4   | ddr_ck_o[0]-          |            | LVSTLD_I_OUT  | PB92B           | BDQ90                                                    |
    | AA13/4   | ddr_cs_o[0]           | LOCATED    | LVSTL_I_OUT   | PB94B           | BDQ90                                                    |
    | AA14/4   |     unused, PULL:DOWN |            |               | PB106A          | PCLKT4_3/BDQ102                                          |
    | AA15/3   | ddr_dq_io[12]         | LOCATED    | LVSTL_I_BIDI  | PB122A          | BDQ126                                                   |
    | AA16/3   | ddr_dq_io[14]         | LOCATED    | LVSTL_I_BIDI  | PB122B          | BDQ126                                                   |
    | AA17/3   |     unused, PULL:DOWN |            |               | PB120B          | ADC_CN13/BDQ114                                          |
    | AA18/3   |     unused, PULL:DOWN |            |               | PB120A          | ADC_CP13/BDQ114                                          |
    | AA19/3   |     unused, PULL:DOWN |            |               | PB146A          | ADC_CP14/BDQ150                                          |
    | AA20/3   |     unused, PULL:DOWN |            |               | PB146B          | ADC_CN14/BDQ150                                          |
    | AA21/3   | ddr_ca_o[2]           | LOCATED    | LVSTL_I_OUT   | PB154B          | PCLKC3_3/LRC_GPLL0T_MFGOUT2/ADC_CN15/BDQ150              |
    | AA22/3   |     unused, PULL:DOWN |            |               | PB150A          | ADC_CP11/BDQS150                                         |
    | AB2/5    |     unused, PULL:DOWN |            |               | PB40A           | PCLKT5_2/BDQ42                                           |
    | AB3/5    |     unused, PULL:DOWN |            |               | PB40B           | PCLKC5_2/BDQ42                                           |
    | AB4/5    |     unused, PULL:DOWN |            |               | PB44B           | BDQ42                                                    |
    | AB5/5    |     unused, PULL:DOWN |            |               | PB46B           | PCLKC5_3/BDQ42                                           |
    | AB6/5    |     unused, PULL:DOWN |            |               | PB48A           | BDQ42                                                    |
    | AB7/4    |     unused, PULL:DOWN |            |               | PB54A           | BDQS54                                                   |
    | AB8/4    |     unused, PULL:DOWN |            |               | PB54B           | BDQSN54                                                  |
    | AB9/4    | ddr_dqs_io[0]+        | LOCATED    | LVSTLD_I_BIDI | PB66A           | BDQS66                                                   |
    | AB10/4   | ddr_dqs_io[0]-        |            | LVSTLD_I_BIDI | PB66B           | BDQSN66                                                  |
    | AB11/4   | ddr_cke_o[0]          | LOCATED    | LVSTL_I_OUT   | PB90A           | BDQS90                                                   |
    | AB12/4   |     unused, PULL:DOWN |            |               | PB90B           | BDQSN90                                                  |
    | AB13/4   |     unused, PULL:DOWN |            |               | PB94A           | BDQ90                                                    |
    | AB14/4   |     unused, PULL:DOWN |            |               | PB102A          | ADC_CP6/BDQS102                                          |
    | AB15/4   |     unused, PULL:DOWN |            |               | PB102B          | ADC_CN6/BDQSN102                                         |
    | AB16/3   | ddr_dqs_io[1]+        | LOCATED    | LVSTLD_I_BIDI | PB126A          | BDQS126                                                  |
    | AB17/3   | ddr_dqs_io[1]-        |            | LVSTLD_I_BIDI | PB126B          | BDQSN126                                                 |
    | AB18/3   |     unused, PULL:DOWN |            |               | PB110A          | VREF3_1/ADC_CP10/BDQ114                                  |
    | AB19/3   | ddr_ca_o[3]           | LOCATED    | LVSTL_I_OUT   | PB110B          | ADC_CN10/BDQ114                                          |
    | AB20/3   | ddr_ca_o[4]           | LOCATED    | LVSTL_I_OUT   | PB114B          | COMP1IN/BDQSN114                                         |
    | AB21/3   | ddr_ca_o[5]           | LOCATED    | LVSTL_I_OUT   | PB114A          | COMP1IP/BDQS114                                          |
    | B1/80    |                       |            |               | SD0_TXDP        |                                                          |
    | B4/80    |                       |            |               | SD2_RXDN        |                                                          |
    | B7/81    |                       |            |               | SD4_RXDN        |                                                          |
    | B8/81    |                       |            |               | SD4_RXDP        |                                                          |
    | B11/81   |                       |            |               | SD5_RXDN        |                                                          |
    | B14/81   |                       |            |               | SD6_RXDP        |                                                          |
    | B17/81   |                       |            |               | SD7_RXDP        |                                                          |
    | B20/83   |                       |            |               | SD_EXT0_REFCLKN |                                                          |
    | B21/83   |                       |            |               | SD_EXT0_REFCLKP |                                                          |
    | B22/83   |                       |            |               | SD_EXT1_REFCLKN |                                                          |
    | C1/80    |                       |            |               | SD0_TXDN        |                                                          |
    | C3/80    |                       |            |               | SD2_RXDP        |                                                          |
    | C5/80    |                       |            |               | SD3_RXDN        |                                                          |
    | C6/80    |                       |            |               | SD3_RXDP        |                                                          |
    | C11/81   |                       |            |               | SD5_RXDP        |                                                          |
    | C13/81   |                       |            |               | SDQ1_REFCLKP    |                                                          |
    | C15/81   |                       |            |               | SD6_RXDN        |                                                          |
    | C17/81   |                       |            |               | SD7_RXDN        |                                                          |
    | C19/0    | Reserved: sysCONFIG   |            |               | PT134A          | INITN                                                    |
    | C20/0    | Reserved: sysCONFIG   |            |               | PT134B          | PROGRAMN                                                 |
    | C21/0    |     unused, PULL:DOWN |            |               | PT140A          | MISO/MD1/SD5/S2_IN/OSC_HI                                |
    | C22/0    |     unused, PULL:DOWN |            |               | PT140B          | MD2/SD6/S2_OUT                                           |
    | D2/80    |                       |            |               | SD0_RXDN        |                                                          |
    | D4/80    |                       |            |               | SD0_REFRET      |                                                          |
    | D6/80    |                       |            |               | SD1_REFRET      |                                                          |
    | D7/80    |                       |            |               | SDQ0_REFCLKP    |                                                          |
    | D9/80    |                       |            |               | SD3_REFRET      |                                                          |
    | D11/81   |                       |            |               | SD5_REFRET      |                                                          |
    | D12/81   |                       |            |               | SDQ1_REFCLKN    |                                                          |
    | D14/81   |                       |            |               | SD7_REXT        |                                                          |
    | D16/81   |                       |            |               | SD7_REFRET      |                                                          |
    | D18/0    |     unused, PULL:DOWN |            |               | PT146A          |                                                          |
    | D19/0    |     unused, PULL:DOWN |            |               | PT146B          |                                                          |
    | D20/0    |     unused, PULL:DOWN |            |               | PT144A          | S7_IN                                                    |
    | D21/0    |     unused, PULL:DOWN |            |               | PT144B          | S7_OUT                                                   |
    | D22/0    |     unused, PULL:DOWN |            |               | PT152A          |                                                          |
    | E1/80    |                       |            |               | SD1_TXDP        |                                                          |
    | E3/80    |                       |            |               | SD0_RXDP        |                                                          |
    | E5/80    |                       |            |               | SD0_REXT        |                                                          |
    | E6/80    |                       |            |               | SD1_REXT        |                                                          |
    | E7/80    |                       |            |               | SDQ0_REFCLKN    |                                                          |
    | E8/80    |                       |            |               | SD2_REFRET      |                                                          |
    | E9/80    |                       |            |               | SD3_REXT        |                                                          |
    | E10/81   |                       |            |               | SD4_REFRET      |                                                          |
    | E12/81   |                       |            |               | SD6_REXT        |                                                          |
    | E13/81   |                       |            |               | SD6_REFRET      |                                                          |
    | E15/0    | Reserved: sysCONFIG   |            |               | PT136B          | DONE/S0_OUT                                              |
    | E16/0    |     unused, PULL:DOWN |            |               | PT142A          | MD3/SD7/S6_IN/OSC_BURST                                  |
    | E17/0    |     unused, PULL:DOWN |            |               | PT142B          | MCSNO/MSDO/S6_OUT                                        |
    | E18/0    |     unused, PULL:DOWN |            |               | PT138B          | MOSI/MD0/SD4/S1_OUT                                      |
    | E21/0    |     unused, PULL:DOWN |            |               | PT154A          |                                                          |
    | E22/0    |     unused, PULL:DOWN |            |               | PT152B          |                                                          |
    | F1/80    |                       |            |               | SD1_TXDN        |                                                          |
    | F8/80    |                       |            |               | SD2_REXT        |                                                          |
    | F10/81   |                       |            |               | SD4_REXT        |                                                          |
    | F12/81   |                       |            |               | SD5_REXT        |                                                          |
    | F15/0    |     unused, PULL:DOWN |            |               | PT136A          | MCLK/PCLKT0_0/S0_IN                                      |
    | F17/0    |     unused, PULL:DOWN |            |               | PT138A          | MCSN/S1_IN/PCLKT0_1                                      |
    | F18/0    |     unused, PULL:DOWN |            |               | PT148B          |                                                          |
    | F19/0    | out_clk1              |            | LVCMOS33_OUT  | PT148A          |                                                          |
    | F20/0    |     unused, PULL:DOWN |            |               | PT150B          |                                                          |
    | F21/0    | uart_txd_o            | LOCATED    | LVCMOS33_OUT  | PT154B          |                                                          |
    | F22/0    | uart_rxd_i            | LOCATED    | LVCMOS33_IN   | PT156A          |                                                          |
    | G2/80    |                       |            |               | SD1_RXDP        |                                                          |
    | G3/80    |                       |            |               | SD1_RXDN        |                                                          |
    | G5/7     | out_clk0              |            | LVCMOS33_OUT  | PL6A            | EIO                                                      |
    | G6/7     |     unused, PULL:DOWN |            |               | PL3B            | EIO                                                      |
    | G7/7     |     unused, PULL:DOWN |            |               | PL3A            | ULC_GPLL0T_IN/EIO                                        |
    | G16/1    |     unused, PULL:DOWN |            |               | PR3B            | S8_IN/EIO                                                |
    | G17/1    |     unused, PULL:DOWN |            |               | PR4A            | URC_GPLL0T_IN/S8_OUT/EIO                                 |
    | G18/1    |     unused, PULL:DOWN |            |               | PR6A            | URC_GPLL0T_MFGOUT1/EIO                                   |
    | G19/1    | Reserved: sysCONFIG   |            |               | PR6B            | TMS/SCSN/URC_GPLL0T_MFGOUT2/S5_IN                        |
    | G20/1    |     unused, PULL:DOWN |            |               | PR11A           | SD3/SDA/USER_SDA/S4_IN                                   |
    | G21/0    |     unused, PULL:DOWN |            |               | PT150A          |                                                          |
    | G22/0    |     unused, PULL:DOWN |            |               | PT156B          |                                                          |
    | H1/7     |     unused, PULL:DOWN |            |               | PL10A           | EIO                                                      |
    | H4/7     |     unused, PULL:DOWN |            |               | PL8B            | EIO                                                      |
    | H5/7     |     unused, PULL:DOWN |            |               | PL8A            | EIO                                                      |
    | H6/7     |     unused, PULL:DOWN |            |               | PL6B            | EIO                                                      |
    | H7/7     |     unused, PULL:DOWN |            |               | PL4B            | ULC_GPLL0T_MFGOUT2/EIO                                   |
    | H8/7     |     unused, PULL:DOWN |            |               | PL4A            | ULC_GPLL0T_MFGOUT1/EIO                                   |
    | H14/1    | mipi_clk              |            | LVCMOS33_OUT  | PR8A            | EIO                                                      |
    | H15/1    | Reserved: sysCONFIG   |            |               | PR8B            | TDI/SSI/SD0/S5_OUT                                       |
    | H16/1    |     unused, PULL:DOWN |            |               | PR4B            | SD10                                                     |
    | H17/1    |     unused, PULL:DOWN |            |               | PR17B           | SD13                                                     |
    | H20/1    |     unused, PULL:DOWN |            |               | PR11B           | SD2/SCL/USER_SCL/S3_IN                                   |
    | H21/1    | Reserved: sysCONFIG   |            |               | PR13A           | TCK/SCLK/PMU_EXT_CLK                                     |
    | H22/1    | rstn_i                | LOCATED    | LVCMOS33_IN   | PR13B           | PMU_WAKEUPN/SD11/S4_OUT                                  |
    | J1/7     | fs[1]                 |            | LVCMOS33_OUT  | PL10B           | EIO                                                      |
    | J2/7     |     unused, PULL:DOWN |            |               | PL15B           | EIO                                                      |
    | J3/7     |     unused, PULL:DOWN |            |               | PL15A           | EIO                                                      |
    | J6/7     | LED[6]                | LOCATED    | LVCMOS33_BIDI | PL13B           | EIO                                                      |
    | J7/7     | LED[4]                | LOCATED    | LVCMOS33_BIDI | PL13A           | EIO                                                      |
    | J8/7     |     unused, PULL:DOWN |            |               | PL11B           | EIO                                                      |
    | J9/7     |     unused, PULL:DOWN |            |               | PL11A           | EIO                                                      |
    | J13/1    |     unused, PULL:DOWN |            |               | PR22A           | EIO                                                      |
    | J14/1    | clk_ext               |            | LVCMOS33_IN   | PR10A           | EIO                                                      |
    | J15/1    | Reserved: sysCONFIG   |            |               | PR10B           | TDO/SSO/SD1/S3_OUT                                       |
    | J16/1    |     unused, PULL:DOWN |            |               | PR15A           | SD9                                                      |
    | J17/1    |     unused, PULL:DOWN |            |               | PR17A           | SD12                                                     |
    | J19/1    |     unused, PULL:DOWN |            |               | PR19B           | SD15                                                     |
    | J20/1    |     unused, PULL:DOWN |            |               | PR19A           | SD14                                                     |
    | J21/1    |     unused, PULL:DOWN |            |               | PR20A           | EIO                                                      |
    | J22/1    |     unused, PULL:DOWN |            |               | PR20B           | EIO                                                      |
    | K1/7     |     unused, PULL:DOWN |            |               | PL22B           | EIO                                                      |
    | K2/7     |     unused, PULL:DOWN |            |               | PL22A           | EIO                                                      |
    | K3/7     |     unused, PULL:DOWN |            |               | PL20B           | EIO                                                      |
    | K4/7     |     unused, PULL:DOWN |            |               | PL20A           | EIO                                                      |
    | K6/7     |     unused, PULL:DOWN |            |               | PL28A           | PCLKT7_2/EIO                                             |
    | K8/7     |     unused, PULL:DOWN |            |               | PL19B           | EIO                                                      |
    | K9/7     |     unused, PULL:DOWN |            |               | PL17B           | EIO                                                      |
    | K10/7    |     unused, PULL:DOWN |            |               | PL17A           | EIO                                                      |
    | K11/1    |     unused, PULL:DOWN |            |               | PR24B           | EIO                                                      |
    | K12/1    |     unused, PULL:DOWN |            |               | PR24A           | EIO                                                      |
    | K13/1    |     unused, PULL:DOWN |            |               | PR22B           | EIO                                                      |
    | K14/1    |     unused, PULL:DOWN |            |               | PR26A           | EIO                                                      |
    | K15/1    |     unused, PULL:DOWN |            |               | PR26B           | EIO                                                      |
    | K17/1    |     unused, PULL:DOWN |            |               | PR15B           | SD8                                                      |
    | K18/1    |     unused, PULL:DOWN |            |               | PR28A           | PCLKT1_2/EIO                                             |
    | K19/1    |     unused, PULL:DOWN |            |               | PR28B           | EIO                                                      |
    | K20/1    |     unused, PULL:DOWN |            |               | PR29A           | PCLKT1_1/EIO                                             |
    | K21/1    |     unused, PULL:DOWN |            |               | PR29B           | EIO                                                      |
    | K22/1    |     unused, PULL:DOWN |            |               | PR38A           | EIO                                                      |
    | L1/7     |     unused, PULL:DOWN |            |               | PL33A           | EIO                                                      |
    | L2/7     |     unused, PULL:DOWN |            |               | PL31B           | EIO                                                      |
    | L3/7     |     unused, PULL:DOWN |            |               | PL31A           | PCLKT7_0/EIO                                             |
    | L4/7     |     unused, PULL:DOWN |            |               | PL29B           | EIO                                                      |
    | L5/7     |     unused, PULL:DOWN |            |               | PL29A           | PCLKT7_1/EIO                                             |
    | L6/7     |     unused, PULL:DOWN |            |               | PL28B           | EIO                                                      |
    | L8/7     |     unused, PULL:DOWN |            |               | PL19A           | EIO                                                      |
    | L9/7     | LED[2]                | LOCATED    | LVCMOS33_BIDI | PL26A           | EIO                                                      |
    | L10/7    | LED[0]                | LOCATED    | LVCMOS33_BIDI | PL24B           | EIO                                                      |
    | L11/7    | LED[7]                | LOCATED    | LVCMOS33_BIDI | PL24A           | EIO                                                      |
    | L12/2    | LED[5]                | LOCATED    | LVCMOS33_BIDI | PR42A           | PCLKT2_0/EIO                                             |
    | L13/2    | LED[1]                | LOCATED    | LVCMOS33_BIDI | PR40B           | EIO                                                      |
    | L14/2    | LED[3]                | LOCATED    | LVCMOS33_BIDI | PR40A           | EIO                                                      |
    | L15/1    |     unused, PULL:DOWN |            |               | PR31B           | EIO                                                      |
    | L16/1    |     unused, PULL:DOWN |            |               | PR31A           | PCLKT1_0/EIO                                             |
    | L18/1    |     unused, PULL:DOWN |            |               | PR33A           | EIO                                                      |
    | L19/1    |     unused, PULL:DOWN |            |               | PR33B           | EIO                                                      |
    | L20/1    |     unused, PULL:DOWN |            |               | PR35A           | EIO                                                      |
    | L21/1    |     unused, PULL:DOWN |            |               | PR35B           | EIO                                                      |
    | L22/1    | init_done_o           |            | LVCMOS33_OUT  | PR38B           | EIO                                                      |
    | M1/7     | gnd_clk               |            | LVCMOS33_OUT  | PL33B           | EIO                                                      |
    | M2/7     |     unused, PULL:DOWN |            |               | PL35A           | EIO                                                      |
    | M3/7     | ddr_odt_ca_o          |            | LVCMOS33_OUT  | PL35B           | EIO                                                      |
    | M4/7     | fs[0]                 |            | LVCMOS33_OUT  | PL38A           | EIO                                                      |
    | M5/7     | LED[8]                |            | LVCMOS33_BIDI | PL38B           | EIO                                                      |
    | M6/6     | LED[9]                |            | LVCMOS33_BIDI | PL40A           | EIO                                                      |
    | M7/6     |     unused, PULL:DOWN |            |               | PL40B           | EIO                                                      |
    | M8/7     |     unused, PULL:DOWN |            |               | PL26B           | EIO                                                      |
    | M9/6     |     unused, PULL:DOWN |            |               | PL51A           | EIO                                                      |
    | M10/6    |     unused, PULL:DOWN |            |               | PL42A           | PCLKT6_0/EIO                                             |
    | M11/6    |     unused, PULL:DOWN |            |               | PL42B           | EIO                                                      |
    | M12/2    |     unused, PULL:DOWN |            |               | PR42B           | EIO                                                      |
    | M13/2    |     unused, PULL:DOWN |            |               | PR49B           | EIO                                                      |
    | M14/2    |     unused, PULL:DOWN |            |               | PR49A           | EIO                                                      |
    | M15/2    |     unused, PULL:DOWN |            |               | PR56B           | EIO                                                      |
    | M16/2    |     unused, PULL:DOWN |            |               | PR56A           | EIO                                                      |
    | M17/2    | cmos_xclr             |            | LVCMOS33_OUT  | PR47A           | EIO                                                      |
    | M18/2    |     unused, PULL:DOWN |            |               | PR47B           | EIO                                                      |
    | M20/2    |     unused, PULL:DOWN |            |               | PR46A           | PCLKT2_2/EIO                                             |
    | M21/2    |     unused, PULL:DOWN |            |               | PR44B           | EIO                                                      |
    | M22/2    |     unused, PULL:DOWN |            |               | PR44A           | PCLKT2_1/EIO                                             |
    | N1/6     |     unused, PULL:DOWN |            |               | PL44A           | PCLKT6_1/EIO                                             |
    | N2/6     |     unused, PULL:DOWN |            |               | PL44B           | EIO                                                      |
    | N3/6     |     unused, PULL:DOWN |            |               | PL46A           | PCLKT6_2/EIO                                             |
    | N4/6     |     unused, PULL:DOWN |            |               | PL46B           | EIO                                                      |
    | N5/6     |     unused, PULL:DOWN |            |               | PL47A           | EIO                                                      |
    | N6/6     |     unused, PULL:DOWN |            |               | PL47B           | EIO                                                      |
    | N7/6     |     unused, PULL:DOWN |            |               | PL49A           | EIO                                                      |
    | N8/6     |     unused, PULL:DOWN |            |               | PL49B           | EIO                                                      |
    | N9/6     |     unused, PULL:DOWN |            |               | PL51B           | EIO                                                      |
    | N10/6    |     unused, PULL:DOWN |            |               | PL58A           | EIO                                                      |
    | N11/2    |     unused, PULL:DOWN |            |               | PR51A           | EIO                                                      |
    | N12/2    |     unused, PULL:DOWN |            |               | PR51B           | EIO                                                      |
    | N13/2    |     unused, PULL:DOWN |            |               | PR53A           | EIO                                                      |
    | N14/2    |     unused, PULL:DOWN |            |               | PR53B           | EIO                                                      |
    | N17/2    |     unused, PULL:DOWN |            |               | PR55A           | EIO                                                      |
    | N18/2    |     unused, PULL:DOWN |            |               | PR55B           | EIO                                                      |
    | N20/2    |     unused, PULL:DOWN |            |               | PR46B           | EIO                                                      |
    | N21/2    |     unused, PULL:DOWN |            |               | PR58B           | EIO                                                      |
    | N22/2    |     unused, PULL:DOWN |            |               | PR58A           | EIO                                                      |
    | P1/6     |     unused, PULL:DOWN |            |               | PL53A           | EIO                                                      |
    | P2/6     |     unused, PULL:DOWN |            |               | PL53B           | EIO                                                      |
    | P3/6     |     unused, PULL:DOWN |            |               | PL55A           | EIO                                                      |
    | P4/6     |     unused, PULL:DOWN |            |               | PL55B           | EIO                                                      |
    | P8/6     |     unused, PULL:DOWN |            |               | PL56B           | EIO                                                      |
    | P9/6     |     unused, PULL:DOWN |            |               | PL56A           | EIO                                                      |
    | P10/6    |     unused, PULL:DOWN |            |               | PL58B           | EIO                                                      |
    | P13/2    |     unused, PULL:DOWN |            |               | PR65A           | EIO                                                      |
    | P14/2    |     unused, PULL:DOWN |            |               | PR65B           | EIO                                                      |
    | P18/2    |     unused, PULL:DOWN |            |               | PR64B           | EIO                                                      |
    | P19/2    |     unused, PULL:DOWN |            |               | PR64A           | EIO                                                      |
    | P20/2    |     unused, PULL:DOWN |            |               | PR62A           | EIO                                                      |
    | P21/2    |     unused, PULL:DOWN |            |               | PR60B           | EIO                                                      |
    | P22/2    |     unused, PULL:DOWN |            |               | PR60A           | EIO                                                      |
    | R1/6     | LED[10]               |            | LVCMOS33_BIDI | PL60A           | EIO                                                      |
    | R2/6     |     unused, PULL:DOWN |            |               | PL60B           | EIO                                                      |
    | R3/6     |     unused, PULL:DOWN |            |               | PL62A           | EIO                                                      |
    | R4/6     |     unused, PULL:DOWN |            |               | PL62B           | EIO                                                      |
    | R5/6     | sim_o                 |            | LVCMOS33_OUT  | PL64A           | EIO                                                      |
    | R6/6     |     unused, PULL:DOWN |            |               | PL64B           | EIO                                                      |
    | R7/6     | LED[11]               |            | LVCMOS33_BIDI | PL65A           | EIO                                                      |
    | R8/6     |     unused, PULL:DOWN |            |               | PL67A           | EIO                                                      |
    | R9/6     | fs[2]                 |            | LVCMOS33_OUT  | PL67B           | EIO                                                      |
    | R14/70   |                       |            |               | ADC_DP0         |                                                          |
    | R15/70   |                       |            |               | ADC_DN0         |                                                          |
    | R16/70   |                       |            |               | ADC_DP1         |                                                          |
    | R17/70   |                       |            |               | ADC_DN1         |                                                          |
    | R20/2    |     unused, PULL:DOWN |            |               | PR62B           | EIO                                                      |
    | R21/2    |     unused, PULL:DOWN |            |               | PR67B           | EIO                                                      |
    | R22/2    |     unused, PULL:DOWN |            |               | PR67A           | EIO                                                      |
    | T1/5     |     unused, PULL:DOWN |            |               | PB6A            | BDQS6                                                    |
    | T2/5     | pll_refclk_i+         | LOCATED    | LVSTLD_I_IN   | PB2A            | LLC_GPLL0T_IN/CDR_RXP0/VREF5_1/ADC_CP0/COMP1P/BDQ6       |
    | T3/5     |     unused, PULL:DOWN |            |               | PB10B           | PCLKC5_1/CDR0_TESTN/ADC_CN2/COMP3N/BDQ6                  |
    | T4/5     |     unused, PULL:DOWN |            |               | PB8A            | ADC_CP3/BDQ6                                             |
    | T5/5     |     unused, PULL:DOWN |            |               | PB4B            | PCLKC5_0/LLC_GPLL0T_MFGOUT2/CDR_RXN1/ADC_CN1/COMP2N/BDQ6 |
    | T6/5     |     unused, PULL:DOWN |            |               | PB12A           | CDR1_TESTP/BDQ6                                          |
    | T7/6     |     unused, PULL:DOWN |            |               | PL65B           | EIO                                                      |
    | T8/4     |     unused, PULL:DOWN |            |               | PB56A           | BDQ54                                                    |
    | T9/4     | ddr_dq_io[0]          | LOCATED    | LVSTL_I_BIDI  | PB64B           | BDQ66                                                    |
    | T10/4    | ddr_dq_io[1]          | LOCATED    | LVSTL_I_BIDI  | PB80B           | BDQ66                                                    |
    | T12/4    |     unused, PULL:DOWN |            |               | PB100B          | PCLKC4_2/ADC_CN7/BDQ102                                  |
    | T14/4    |     unused, PULL:DOWN |            |               | PB108B          | VREF4_2/BDQ102                                           |
    | T15/3    |     unused, PULL:DOWN |            |               | PB130B          | BDQ126                                                   |
    | T16/3    |     unused, PULL:DOWN |            |               | PB136A          | BDQ138                                                   |
    | T17/3    |     unused, PULL:DOWN |            |               | PB140A          | BDQ138                                                   |
    | T18/3    |     unused, PULL:DOWN |            |               | PB144A          | BDQ138                                                   |
    | T19/3    |     unused, PULL:DOWN |            |               | PB134A          | BDQ138                                                   |
    | T20/3    |     unused, PULL:DOWN |            |               | PB142A          | BDQ138                                                   |
    | T21/3    |     unused, PULL:DOWN |            |               | PB142B          | BDQ138                                                   |
    | T22/3    |     unused, PULL:DOWN |            |               | PB138A          | BDQS138                                                  |
    | U1/5     |     unused, PULL:DOWN |            |               | PB6B            | BDQSN6                                                   |
    | U2/5     | pll_refclk_i-         |            | LVSTLD_I_IN   | PB2B            | LLC_GPLL0C_IN/CDR_RXN0/ADC_CN0/COMP1N/BDQ6               |
    | U3/5     |     unused, PULL:DOWN |            |               | PB10A           | PCLKT5_1/CDR0_TESTP/ADC_CP2/COMP3P/BDQ6                  |
    | U4/5     |     unused, PULL:DOWN |            |               | PB8B            | ADC_CN3/BDQ6                                             |
    | U5/5     |     unused, PULL:DOWN |            |               | PB4A            | PCLKT5_0/LLC_GPLL0T_MFGOUT1/CDR_RXP1/ADC_CP1/COMP2P/BDQ6 |
    | U6/5     |     unused, PULL:DOWN |            |               | PB12B           | CDR1_TESTN/BDQ6                                          |
    | U7/4     |     unused, PULL:DOWN |            |               | PB52B           | PCLKC4_0/BDQ54                                           |
    | U8/4     |     unused, PULL:DOWN |            |               | PB56B           | BDQ54                                                    |
    | U9/4     |     unused, PULL:DOWN |            |               | PB64A           | BDQ66                                                    |
    | U10/4    | ddr_dq_io[2]          | LOCATED    | LVSTL_I_BIDI  | PB80A           | BDQ66                                                    |
    | U11/4    |     unused, PULL:DOWN |            |               | PB86A           | BDQ90                                                    |
    | U12/4    |     unused, PULL:DOWN |            |               | PB100A          | PCLKT4_2/ADC_CP7/BDQ102                                  |
    | U13/4    |     unused, PULL:DOWN |            |               | PB104B          | ADC_CN9/BDQ102                                           |
    | U14/4    |     unused, PULL:DOWN |            |               | PB108A          | BDQ102                                                   |
    | U15/3    | ddr_dmi_io[1]         | LOCATED    | LVSTL_I_BIDI  | PB130A          | BDQ126                                                   |
    | U16/3    |     unused, PULL:DOWN |            |               | PB136B          | BDQ138                                                   |
    | U17/3    |     unused, PULL:DOWN |            |               | PB140B          | BDQ138                                                   |
    | U18/3    |     unused, PULL:DOWN |            |               | PB144B          | BDQ138                                                   |
    | U19/3    |     unused, PULL:DOWN |            |               | PB134B          | BDQ138                                                   |
    | U20/3    |     unused, PULL:DOWN |            |               | PB156A          | LRC_GPLL0T_IN/ATB_FORCE/BDQ150                           |
    | U21/3    |     unused, PULL:DOWN |            |               | PB156B          | LRC_GPLL0C_IN/VREF3_2/ATB_SENSE/BDQ150                   |
    | U22/3    |     unused, PULL:DOWN |            |               | PB138B          | BDQSN138                                                 |
    | V1/5     |     unused, PULL:DOWN |            |               | PB30A           | BDQS30                                                   |
    | V5/5     |     unused, PULL:DOWN |            |               | PB36B           | BDQ30                                                    |
    | V6/5     |     unused, PULL:DOWN |            |               | PB36A           | BDQ30                                                    |
    | V7/4     |     unused, PULL:DOWN |            |               | PB52A           | PCLKT4_0/BDQ54                                           |
    | V8/4     |     unused, PULL:DOWN |            |               | PB60B           | BDQ54                                                    |
    | V10/4    | ddr_dq_io[6]          | LOCATED    | LVSTL_I_BIDI  | PB84B           | BDQ66                                                    |
    | V11/4    |     unused, PULL:DOWN |            |               | PB86B           | BDQ90                                                    |
    | V13/4    |     unused, PULL:DOWN |            |               | PB104A          | ADC_CP9/BDQ102                                           |
    | V14/4    |     unused, PULL:DOWN |            |               | PB98A           | ADC_CP5/BDQ102                                           |
    | V15/3    | ddr_dq_io[15]         | LOCATED    | LVSTL_I_BIDI  | PB128A          | BDQ126                                                   |
    | V16/3    | ddr_dq_io[10]         | LOCATED    | LVSTL_I_BIDI  | PB132B          | BDQ126                                                   |
    | V18/3    |     unused, PULL:DOWN |            |               | PB118B          | PCLKC3_1/COMP2IN/BDQ114                                  |
    | V19/3    |     unused, PULL:DOWN |            |               | PB118A          | PCLKT3_1/COMP2IP/BDQ114                                  |
    | V21/3    |     unused, PULL:DOWN |            |               | PB152B          | ADC_CN12/BDQ150                                          |
    | V22/3    |     unused, PULL:DOWN |            |               | PB152A          | ADC_CP12/BDQ150                                          |
    | W1/5     |     unused, PULL:DOWN |            |               | PB30B           | BDQSN30                                                  |
    | W2/5     |     unused, PULL:DOWN |            |               | PB34A           | BDQ30                                                    |
    | W3/5     |     unused, PULL:DOWN |            |               | PB26A           | BDQ30                                                    |
    | W5/5     |     unused, PULL:DOWN |            |               | PB28A           | BDQ30                                                    |
    | W6/5     |     unused, PULL:DOWN |            |               | PB32A           | BDQ30                                                    |
    | W7/4     | ddr_ca_o[1]           | LOCATED    | LVSTL_I_OUT   | PB50A           | VREF4_1/BDQ54                                            |
    | W8/4     |     unused, PULL:DOWN |            |               | PB60A           | BDQ54                                                    |
    | W10/4    | ddr_dq_io[5]          | LOCATED    | LVSTL_I_BIDI  | PB84A           | BDQ66                                                    |
    | W11/4    |     unused, PULL:DOWN |            |               | PB88B           | BDQ90                                                    |
    | W13/4    |     unused, PULL:DOWN |            |               | PB96B           | BDQ90                                                    |
    | W14/4    |     unused, PULL:DOWN |            |               | PB98B           | ADC_CN5/BDQ102                                           |
    | W15/3    | ddr_dq_io[9]          | LOCATED    | LVSTL_I_BIDI  | PB128B          | BDQ126                                                   |
    | W16/3    | ddr_dq_io[11]         | LOCATED    | LVSTL_I_BIDI  | PB132A          | BDQ126                                                   |
    | W18/3    |     unused, PULL:DOWN |            |               | PB116B          | ADC_CN8/BDQ114                                           |
    | W19/3    |     unused, PULL:DOWN |            |               | PB116A          | ADC_CP8/BDQ114                                           |
    | W21/3    |     unused, PULL:DOWN |            |               | PB148B          | PCLKC3_2/COMP3IN/BDQ150                                  |
    | W22/3    |     unused, PULL:DOWN |            |               | PB148A          | PCLKT3_2/COMP3IP/BDQ150                                  |
    | Y1/5     |     unused, PULL:DOWN |            |               | PB42A           | BDQS42                                                   |
    | Y2/5     |     unused, PULL:DOWN |            |               | PB34B           | BDQ30                                                    |
    | Y3/5     |     unused, PULL:DOWN |            |               | PB26B           | BDQ30                                                    |
    | Y5/5     |     unused, PULL:DOWN |            |               | PB28B           | BDQ30                                                    |
    | Y6/5     |     unused, PULL:DOWN |            |               | PB32B           | BDQ30                                                    |
    | Y7/4     | ddr_ca_o[0]           | LOCATED    | LVSTL_I_OUT   | PB50B           | BDQ54                                                    |
    | Y8/4     |     unused, PULL:DOWN |            |               | PB58B           | PCLKC4_1/BDQ54                                           |
    | Y10/4    | ddr_dq_io[7]          | LOCATED    | LVSTL_I_BIDI  | PB82B           | BDQ66                                                    |
    | Y11/4    |     unused, PULL:DOWN |            |               | PB88A           | BDQ90                                                    |
    | Y13/4    |     unused, PULL:DOWN |            |               | PB96A           | BDQ90                                                    |
    | Y14/4    |     unused, PULL:DOWN |            |               | PB106B          | PCLKC4_3/BDQ102                                          |
    | Y15/3    | ddr_dq_io[13]         | LOCATED    | LVSTL_I_BIDI  | PB124A          | BDQ126                                                   |
    | Y16/3    | ddr_dq_io[8]          | LOCATED    | LVSTL_I_BIDI  | PB124B          | BDQ126                                                   |
    | Y18/3    |     unused, PULL:DOWN |            |               | PB112B          | PCLKC3_0/ADC_CN4/BDQ114                                  |
    | Y19/3    |     unused, PULL:DOWN |            |               | PB112A          | PCLKT3_0/ADC_CP4/BDQ114                                  |
    | Y21/3    | ddr_reset_n_o         | LOCATED    | LVSTL_I_OUT   | PB154A          | PCLKT3_3/LRC_GPLL0T_MFGOUT1/ADC_CP15/BDQ150              |
    | Y22/3    |     unused, PULL:DOWN |            |               | PB150B          | ADC_CN11/BDQSN150                                        |
    +----------+-----------------------+------------+---------------+-----------------+----------------------------------------------------------+

    sysCONFIG Pins:
    +----------+-----------------------------------+----------+-------------+
    | Pad Name | sysCONFIG Pin Name                | Pin/Bank | Buffer Type |
    +----------+-----------------------------------+----------+-------------+
    | PT134A   | INITN                             | C19/0    |             |
    | PT134B   | PROGRAMN                          | C20/0    |             |
    | PT136B   | DONE/S0_OUT                       | E15/0    |             |
    | PR13A    | TCK/SCLK/PMU_EXT_CLK              | H21/1    |             |
    | PR10B    | TDO/SSO/SD1/S3_OUT                | J15/1    |             |
    | PR8B     | TDI/SSI/SD0/S5_OUT                | H15/1    |             |
    | PR6B     | TMS/SCSN/URC_GPLL0T_MFGOUT2/S5_IN | G19/1    |             |
    +----------+-----------------------------------+----------+-------------+

    Locate Constraints for each Pin:

    ldc_set_location -site {L10} [ get_ports {LED[0]} ]
    ldc_set_location -site {R1} [ get_ports {LED[10]} ]
    ldc_set_location -site {R7} [ get_ports {LED[11]} ]
    ldc_set_location -site {L13} [ get_ports {LED[1]} ]
    ldc_set_location -site {L9} [ get_ports {LED[2]} ]
    ldc_set_location -site {L14} [ get_ports {LED[3]} ]
    ldc_set_location -site {J7} [ get_ports {LED[4]} ]
    ldc_set_location -site {L12} [ get_ports {LED[5]} ]
    ldc_set_location -site {J6} [ get_ports {LED[6]} ]
    ldc_set_location -site {L11} [ get_ports {LED[7]} ]
    ldc_set_location -site {M5} [ get_ports {LED[8]} ]
    ldc_set_location -site {M6} [ get_ports {LED[9]} ]
    ldc_set_location -site {J14} [ get_ports {clk_ext} ]
    ldc_set_location -site {M17} [ get_ports {cmos_xclr} ]
    ldc_set_location -site {Y7} [ get_ports {ddr_ca_o[0]} ]
    ldc_set_location -site {W7} [ get_ports {ddr_ca_o[1]} ]
    ldc_set_location -site {AA21} [ get_ports {ddr_ca_o[2]} ]
    ldc_set_location -site {AB19} [ get_ports {ddr_ca_o[3]} ]
    ldc_set_location -site {AB20} [ get_ports {ddr_ca_o[4]} ]
    ldc_set_location -site {AB21} [ get_ports {ddr_ca_o[5]} ]
    ldc_set_location -site {AA11} [ get_ports {ddr_ck_o[0]} ]
    ldc_set_location -site {AB11} [ get_ports {ddr_cke_o[0]} ]
    ldc_set_location -site {AA13} [ get_ports {ddr_cs_o[0]} ]
    ldc_set_location -site {AA8} [ get_ports {ddr_dmi_io[0]} ]
    ldc_set_location -site {U15} [ get_ports {ddr_dmi_io[1]} ]
    ldc_set_location -site {T9} [ get_ports {ddr_dq_io[0]} ]
    ldc_set_location -site {V16} [ get_ports {ddr_dq_io[10]} ]
    ldc_set_location -site {W16} [ get_ports {ddr_dq_io[11]} ]
    ldc_set_location -site {AA15} [ get_ports {ddr_dq_io[12]} ]
    ldc_set_location -site {Y15} [ get_ports {ddr_dq_io[13]} ]
    ldc_set_location -site {AA16} [ get_ports {ddr_dq_io[14]} ]
    ldc_set_location -site {V15} [ get_ports {ddr_dq_io[15]} ]
    ldc_set_location -site {T10} [ get_ports {ddr_dq_io[1]} ]
    ldc_set_location -site {U10} [ get_ports {ddr_dq_io[2]} ]
    ldc_set_location -site {AA9} [ get_ports {ddr_dq_io[3]} ]
    ldc_set_location -site {AA10} [ get_ports {ddr_dq_io[4]} ]
    ldc_set_location -site {W10} [ get_ports {ddr_dq_io[5]} ]
    ldc_set_location -site {V10} [ get_ports {ddr_dq_io[6]} ]
    ldc_set_location -site {Y10} [ get_ports {ddr_dq_io[7]} ]
    ldc_set_location -site {Y16} [ get_ports {ddr_dq_io[8]} ]
    ldc_set_location -site {W15} [ get_ports {ddr_dq_io[9]} ]
    ldc_set_location -site {AB9} [ get_ports {ddr_dqs_io[0]} ]
    ldc_set_location -site {AB16} [ get_ports {ddr_dqs_io[1]} ]
    ldc_set_location -site {M3} [ get_ports {ddr_odt_ca_o} ]
    ldc_set_location -site {Y21} [ get_ports {ddr_reset_n_o} ]
    ldc_set_location -site {M4} [ get_ports {fs[0]} ]
    ldc_set_location -site {J1} [ get_ports {fs[1]} ]
    ldc_set_location -site {R9} [ get_ports {fs[2]} ]
    ldc_set_location -site {M1} [ get_ports {gnd_clk} ]
    ldc_set_location -site {L22} [ get_ports {init_done_o} ]
    ldc_set_location -site {H14} [ get_ports {mipi_clk} ]
    ldc_set_location -site {G5} [ get_ports {out_clk0} ]
    ldc_set_location -site {F19} [ get_ports {out_clk1} ]
    ldc_set_location -site {T2} [ get_ports {pll_refclk_i} ]
    ldc_set_location -site {H22} [ get_ports {rstn_i} ]
    ldc_set_location -site {R5} [ get_ports {sim_o} ]
    ldc_set_location -site {F22} [ get_ports {uart_rxd_i} ]
    ldc_set_location -site {F21} [ get_ports {uart_txd_o} ]

    #PLL
    ldc_set_location -site {PLL_LLC} [ get_cells {u_mem/lscc_lpddr4_mc_inst/u_lp4mem/u_pll/gen_no_refclk_mon.u_PLL.PLL_inst} ]
    # ldc_set_location -site {PLL_LLC} [ get_cells {u_mem.lscc_lpddr4_mc_inst.u_lp4mem.u_pll.gen_no_refclk_mon.u_PLL.PLL_inst} ]
    #DQSDLL
    ldc_set_location -site {DDRDLL_CORE_R72C158} [ get_cells {u_mem.lscc_lpddr4_mc_inst.u_lp4mem.u1_clock_sync.u0_DDRDLL.DDRDLL_inst} ]
    #PLL
    ldc_set_location -site {PLL_ULC} [ get_cells {ASYNC_AXI.u_aclk_pclk/lscc_pll_inst/gen_no_refclk_mon.u_PLL.PLL_inst} ]
    # ldc_set_location -site {PLL_ULC} [ get_cells {ASYNC_AXI.u_aclk_pclk.lscc_pll_inst.gen_no_refclk_mon.u_PLL.PLL_inst} ]

    Copyright (c) 2002-2022 Lattice Semiconductor Corporation,  All rights reserved.

    Mon Mar 18 12:42:55 2024